**Section § 396.3: Inspection, repair and maintenance.**

Below are the available interpretations for the given section. To return to the list of parts, use the Parts link above. The menu to the left provides a full list of sections that have interpretations. To view interpretations for a different section, click on the menu item.

The regulations text of the section can be found on the eCFR website. To view the regulations text, use the link below.

## Guidance Q&A

**Question 2: § 396.3(b)(4) refers to a record of tests. What tests are required of push-out windows and emergency door lamps on buses?**

**Guidance:** Generally, inspection of a push-out window would require pushing out the window. However, if the window may be destroyed by pushing out to test its proper functioning, a visual inspection may qualify as a test if the inspector can ascertain the proper functioning of the window without opening it. Checking to ensure that the rubber push-out molding is properly in place and has not deteriorated and that any handles or marking instructions have not been tampered with would meet the test requirement. Inspection of emergency door marking lights would require opening the door to test the lights.