Editorial Category: ELDS

Editorial Type … Significant Regulatory Guidance

Unique Identifier: FMCSA-HOS-ELD-TECH-395-FAQ25

Mode: Trucking

Topic: ELDS

Subject: Technology

Keywords: Electronic logging device, ELD, functional specifications, Appendix A, ELD Technical Specifications, Data, Recording, engine hours, ECM, aggregate total, 31137

Tags: Electronic logging device, ELD, functional specifications, Appendix A, ELD Technical Specifications, Data, Recording, engine hours, ECM, aggregate total, 31137

**Word.docx (***ELD Tech FAQ25***)**

**Description**

**Frequently Asked Questions: Electronic Logging Devices and Hours of Service – Technical Specifications**

##### Question 25: If the vehicle does not track engine hours, can the record begin with “0”?

If it is not possible to obtain the engine hours from the ECM, then the ELD may begin recording engine hours at “0” for the given engine the first time the ELD is used with that engine. After the first use, the ELD must continue to keep and use an aggregate total from the first time it was installed or used with an engine. Ideally, back office systems can share this aggregate total so that any other ELD used with the engine can start at the aggregate total, rather than “0.”

**Contact Info**

ELD@dot.gov

#### Effective Date

September 2017

#### Issued Date

September 2017

|  |  |  |
| --- | --- | --- |
| Program Review |  |  |
| Legal Review | Amanda Burgie |  |
|  |  |  |
| Modified from original guidance | No |  |
| Other information |  |  |