Editorial Category: ELDS

Editorial Type … Significant Regulatory Guidance

Unique Identifier: FMCSA-HOS-ELD-TECH-395-FAQ28

Mode: Trucking

Topic: ELDS

Subject: Technology

Keywords: Electronic logging device, ELD, functional specifications, Appendix A, ELD Technical Specifications, Data, Recording, portable device, platform, sequence number, event identifier, black box, 31137

Tags: Electronic logging device, ELD, functional specifications, Appendix A, ELD Technical Specifications, Data, Recording, portable device, platform, sequence number, event identifier, black box, 31137

**Word.docx (***ELD Tech FAQ28***)**

**Description**

**Frequently Asked Questions: Electronic Logging Devices and Hours of Service – Technical Specifications**

##### Question 28: In a portable device platform, should the event identifier sequence number be associated with the portable device or the vehicle’s black box?

The ELD Rule requires that the event identifier sequence number be consistently applied. It does not specify if the event identifier sequence number must be associated with the portable device or the vehicle’s black box, this is left to the discretion of the provider.

**Contact Info**

ELD@dot.gov

#### Effective Date

September 2017

#### Issued Date

September 2017

|  |  |  |
| --- | --- | --- |
| Program Review |  |  |
| Legal Review | Amanda Burgie |  |
|  |  |  |
| Modified from original guidance | No |  |
| Other information |  |  |