Editorial Category: ELDS

Editorial Type … Significant Regulatory Guidance

Unique Identifier: FMCSA-HOS-ELD-TECH-395-FAQ29

Mode: Trucking

Topic: ELDS

Subject: Technology

Keywords: Electronic logging device, ELD, functional specifications, Appendix A, ELD Technical Specifications, Data, Recording, 31137, inactive, replacement record, existing record, active, sequence ID, sequence ID number, edit

Tags: Electronic logging device, ELD, functional specifications, Appendix A, ELD Technical Specifications, Data, Recording, 31137, inactive, replacement record, existing record, active, sequence ID, sequence ID number, edit

**Word.docx (***ELD Tech FAQ29***)**

**Description**

**Frequently Asked Questions: Electronic Logging Devices and Hours of Service – Technical Specifications**

##### Question 29: When an existing record becomes inactive and its replacement record becomes active or inactive‐ change‐requested, is it acceptable that the replacement record has the same sequence ID as the record it replaces?

No, the replacement record must have its own sequence ID number.

When a driver edits an event or a motor carrier suggests an edit, the new event record should have a new sequence ID number.

**Contact Info**

ELD@dot.gov

#### Effective Date

September 2017

#### Issued Date

September 2017

|  |  |  |
| --- | --- | --- |
| Program Review |  |  |
| Legal Review | Amanda Burgie |  |
|  |  |  |
| Modified from original guidance | No |  |
| Other information |  |  |