**Section § 393.60: Glazing in specified openings.**

## Guidance Q&A

**Question 1: May windshields and side windows be tinted?**

**Guidance:** Yes, as long as the light transmission is not restricted to less than 70 percent of normal (refer to the American Standards Association publication Z26.1-1966 and Z26.1a-1969).

|  |  |  |
| --- | --- | --- |
| Program Review |  |  |
|  |  |  |
| Legal Review | Charles Medalen | 2/20/20 |
|  |  |  |
| Modified from original guidance |  |  |
| Other information |  |  |