**Section § 393.104: What standards must cargo securement devices and systems meet in order to satisfy the requirements of this subpart?**

## Guidance Q&A

**Question 2: Does § 393.104(b) require that securement devices be marked or labeled with their working load limit or any other information?**

**Guidance:** No. Although § 393.104(b) requires chain, wire rope, synthetic webbing, cordage, and steel strapping tiedowns to meet applicable manufacturing standards, it explicitly excludes marking identification provisions of those manufacturing standards. Since § 393.104(b) does not establish manufacturing standards or marking requirements for other types of securement devices, such devices are not required to be marked with their working load limit.