**Section § 393.48: Brakes to be operative.**

## Guidance Q&A

**Question 1: If a CMV manufactured on or after July 25, 1980 (see § 393.42) has brake components on the front axle, and the brakes are not operable, does the vehicle comply with § 393.48?**