**Section § 393.83: Exhaust systems.**

## Guidance Q&A

**Question 1: Is a heat shield mandatory on a vertical exhaust stack?**

**Guidance:** No. However, § 393.83 requires the placement of the exhaust system in such a manner as to prevent the burning, charring, or damaging of the electrical wiring, the fuel supply, or any combustible part of the CMV.