FMCSA-ELD-395-Q035(2022-03-10)

**Question:** Can the partial vehicle identification number (VIN) value obtained from the controller area network bus be used for reporting?

**Guidance**: Partial VIN is not permitted. If the VIN cannot be fully obtained from the electronic control module (ECM), it may be entered manually; however, a partial VIN broadcast can be used to aid the driver in entering a manual VIN. Please note:

* Providers are encouraged to use the VIN check digit calculation to help prevent user entry errors.
* A VIN with any level of manual entry must be prefixed by a “-” character in the output file.
* Manual VIN entry cannot be used when the complete VIN can be obtained from the ECM. A device using manual entry when the complete VIN is in fact available from the ECM would not be in compliance with the rule and would be subject to removal from the list of self-certified and registered ELDs.

**Contact Info:** FMCSA ELD Information, 1-800-832-5660 or [ELD@dot.gov](mailto:ELD@dot.gov).

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

*Note: This guidance document does not have the force and effect of law and is not meant to bind the public in any way.  It is intended only to provide information and clarity regarding existing requirements under the law or agency policies.*

**Regulatory Topic: ELD Guidance**

Effective Date: Thursday, March 10, 2022

Issued Date: Thursday, March 10, 2022