FMCSA-ELD-395-Q061(2022-03-10)

**Question:** Would server-based events (e.g., edits and assignment of unassigned events) generate a different sequence ID than that generated by the electronic logging device (ELD)?

**Guidance**: The sequence ID must be continuous to its source device. In an ELD support system, that system may have its own sequence ID generator. Because events cannot be deleted, it should be possible to observe each component in the ELD system which generates sequence IDs and find a continuous list of events for each sequence number without any gaps.

**Contact Info:** FMCSA ELD Information, 1-800-832-5660 or ELD@dot.gov.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

*Note: This guidance document does not have the force and effect of law and is not meant to bind the public in any way.  It is intended only to provide information and clarity regarding existing requirements under the law or agency policies.*

**Regulatory Topic: ELD Guidance**

Effective Date: Thursday, March 10, 2022

Issued Date: Thursday, March 10, 2022