**§392.9 Inspection of cargo, cargo securement devices and systems.**

## Guidance Q&A

***Question 3:*** How may the motor carrier determine safe loading when a shipper has loaded and sealed the trailer?

***Guidance****:* Under these circumstances, a motor carrier may fulfill its responsibilities for proper loading a number of ways. Examples are:

a. Arrange for supervision of loading to determine compliance; or

b. Obtain notation on the connecting line freight bill that the lading was properly loaded; or

c. Obtain approval to break the seal to permit inspection.