**§392.9 Inspection of cargo, cargo securement devices and systems.**

## Guidance Q&A

***Question 4:*** Is there a requirement that a driver must personally load, block, brace, and tie down the cargo on the property carrying CMV he/she drives?

***Guidance:*** No. But the driver is required to be familiar with methods and procedures for securing cargo, and may have to adjust the cargo or load securing devices pursuant to §392.9(b).