Editorial Category: ELDS

Editorial Type … Significant Regulatory Guidance

Unique Identifier: FMCSA-HOS-ELD-TECH-395-FAQ24

Mode: Trucking

Topic: ELDS

Subject: Technology

Keywords: Electronic logging device, ELD, functional specifications, Appendix A, ELD Technical Specifications, Data, Recording, odometer, display, dashboard, replaced, sync, ECM, 31137

Tags: Electronic logging device, ELD, functional specifications, Appendix A, ELD Technical Specifications, Data, Recording, odometer, display, dashboard, replaced, sync, ECM, 31137

**Word.docx (***ELD Tech FAQ24***)**

**Description**

**Frequently Asked Questions: Electronic Logging Devices and Hours of Service – Technical Specifications**

##### Question 24: How should the ELD handle the dashboard odometer display not matching the odometer value returned by the ECM? For instance, when the engine is replaced and the value is not synced.

If the dashboard odometer display does not match the odometer value returned by the ECM, the ECM odometer value must be identified as the valid value.

**Contact Info**

ELD@dot.gov

#### Effective Date

September 2017

#### Issued Date

September 2017

|  |  |  |
| --- | --- | --- |
| Program Review |  |  |
| Legal Review | Amanda Burgie |  |
|  |  |  |
| Modified from original guidance | No |  |
| Other information |  |  |