Editorial Category: ELDS

Editorial Type … Significant Regulatory Guidance

Unique Identifier: FMCSA-HOS-ELD-TECH-395-FAQ30

Mode: Trucking

Topic: ELDS

Subject: Technology

Keywords: Electronic logging device, ELD, functional specifications, Appendix A, ELD Technical Specifications, Data, Recording, 31137, 4.9.2, subset, field, safety official

Tags: Electronic logging device, ELD, functional specifications, Appendix A, ELD Technical Specifications, Data, Recording, 31137, 4.9.2, subset, field, safety official

**Word.docx (***ELD Tech FAQ30***)**

**Description**

**Frequently Asked Questions: Electronic Logging Devices and Hours of Service – Technical Specifications**

##### Question 30: When creating an ELD file as specified in Section 4.9.2, when a field specifies activities on a per‐CMV basis (such as engine power‐up and shut‐down activities), which records should be included?

The ELD file referenced in Section 4.9.2 is specific to the file that the motor carrier must provide to the safety official during an investigation. Therefore, any subset of drivers and vehicles, for a subset 6- months specified by an authorized safety official must be included.

**Contact Info**

ELD@dot.gov

#### Effective Date

September 2017

#### Issued Date

September 2017

|  |  |  |
| --- | --- | --- |
| Program Review |  |  |
| Legal Review | Amanda Burgie |  |
|  |  |  |
| Modified from original guidance | No |  |
| Other information |  |  |