Access requirements for truck and truck-tractor cabs

**Part 399**

**§ 399.207 Truck and truck-tractor access requirements**

***Question 4:* Question:**

May the step be a rung? If so, what minimum diameter must the rung be?

*Guidance*: Yes, the step may be a rung. There is no minimum requirement for the diameter of a step rung. However, it must meet the performance requirements in § 399.207(b)(5).