**Section § 396.3: Inspection, repair and maintenance.**

Below are the available interpretations for the given section. To return to the list of parts, use the Parts link above. The menu to the left provides a full list of sections that have interpretations. To view interpretations for a different section, click on the menu item.

The regulations text of the section can be found on the eCFR website. To view the regulations text, use the link below.

## Guidance Q&A

**Question 1: What is meant by ‘‘systematic inspection, repair, and maintenance?”**

**Guidance:** Generally, systematic means a regular or scheduled program to keep vehicles in a safe operating condition. § 396.3 does not specify inspection, maintenance, or repair intervals because such intervals are fleet specific and, in some instances, vehicle specific. The inspection, repair, and maintenance intervals are to be determined by the motor carrier. The requirements of § 396.11, 396.13, and 396.17 are in addition to the systematic inspection, repair, and maintenance required by § 396.3.