**Section § 393.130: What are the rules for securing heavy vehicles, equipment and machinery?**

## Guidance Q&A

**Question 2: How should I secure the accessories for an item of construction equipment which weighs 4,536 kg (10,000 lb.) or more, if the accessory devices would extend beyond the width of the trailer if they are lowered to the deck for transport?**

**Guidance:** The accessory devices (plows, trencher bars, and the like) may be transported in a raised position, provided they are designed to be transported in that manner. However, the accessory equipment must be locked in place for transport to ensure that neither the accessories nor the equipment itself shifts during transport.