**Section § 393.43: Breakaway and emergency braking.**

## Guidance Q&A

**Question 1: Are tractor protection valves required by § 393.43(b), or may similar devices be used?**

**Guidance:** No. Similar devices may be used provided the devices meet the performance requirements of § 393.43(b).