**Section § 393.51: Warning signals, air pressure and vacuum gauges.**

**Guidance Q&A**

**Question 3: Are vacuum gauges required on the vacuum portion of vacuum-assisted hydraulic brakes?**

**Guidance:** No. Section 393.51(d)(2) requires only that CMVs with vacuum brakes (not hydraulic brakes applied or assisted by vacuum) be equipped with a vacuum gauge.