FMCSA-ELD-395-Q070(2022-03-10)

**Question:** How can yard moves be reflected on the electronic logging device (ELD)?

**Guidance**: The ELD must provide an option to preconfigure drivers’ accounts with yard moves. Should the motor carrier opt to preconfigure a driver’s account with yard moves, the driver must select the beginning and end of the yard move period. The graph-grid must overlay periods of driver’s indications of yard moves using a different style line (such as dashed or dotted line) or shading. The appropriate abbreviation must also be indicated on the graph-grid.

**Contact Info:** FMCSA ELD Information, 1-800-832-5660 or ELD@dot.gov.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

*Note: This guidance document does not have the force and effect of law and is not meant to bind the public in any way.  It is intended only to provide information and clarity regarding existing requirements under the law or agency policies.*

**Regulatory Topic: ELD Guidance**

Effective Date: Thursday, March 10, 2022

Issued Date: Thursday, March 10, 2022