FMCSA-HOS-ELD-395-FAQ020(2018-09-19)-CORR1

**Question:** When does the pre-2000 model year exception apply?

**Guidance:** When a vehicle is registered, the model year should follow the criteria established by the National Highway Traffic Safety Administration (NHTSA). Generally, the model year is determined by reviewing the vehicle identification number (VIN) on the vehicle registration. If the model year is pre-2000 based on the VIN, an ELD is not required.

However, there may be instances when the model year reflected on the vehicle registration is not the same as the engine model year, most commonly when a vehicle is rebuilt using a “glider kit” or when an engine is swapped from one vehicle to another. Vehicles with engines predating model year 2000 are also accepted and are not required to have an ELD, even if the VIN reported on the registration indicates that the commercial motor vehicle (CMV) is a later model year. While the driver is not required to possess documentation that confirms the vehicle engine model year, 49 CFR part 379 [Appendix A](https://www.ecfr.gov/current/title-49/subtitle-B/chapter-III/subchapter-B/part-379#Appendix-A-to-Part-379) requires motor carriers to maintain all documentation on motor and engine changes at the principal place of business.

**Contact Info:** FMCSA ELD Information, 1-800-832-5660 or ELD@dot.gov.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

*Note: This guidance document does not have the force and effect of law and is not meant to bind the public in any way. It is intended only to provide information and clarity regarding existing requirements under the law or agency policies.*

**Regulatory Topic: ELD Guidance**

Effective Date: Wednesday, September 19, 2018

Issued Date: Wednesday, September 19, 2018