FMCSA-HOS-ELD-TECH-395-FAQ73(2018-03-05)-CORR1

Question: Can a Canada/Mexico-domiciled motor carrier’s driver manually enter the vehicle identification number (VIN) for the power unit if the ELD is unable to automatically retrieve the VIN from the engine?

**Answer:** Yes. The driver can add the VIN manually if the ELD cannot retrieve the VIN from the vehicle engine data.

**Contact Info:** FMCSA ELD Information, 1-800-832-5660 or ELD@dot.gov.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

*Note: This guidance document does not have the force and effect of law and is not meant to bind the public in any way.  It is intended only to provide information and clarity regarding existing requirements under the law or agency policies.*

**Regulatory Topic: ELD requirements for foreign-domiciled motor carriers**

**Effective Date:** Monday, March 5, 2018

**Issued Date:** Monday, March 5, 2018