FMCSA-HOS-ELD-TECH-395-FAQ56

**Frequently Asked Questions: Electronic Logging Devices and Hours of Service – Technical Specifications**

**Question:**

Under Section 4.8.1.3(c) of Appendix A to Part 395, the graph-grid for each day’s records of duty status must be at least 6 inches by 1.5 inches in size. Can you clarify what this means for requirements for screen size?

**Guidance:**

This size requirement is for print display only, it does not apply to the ELD screen itself.

**Regulatory Topic: ELD Guidance**

Effective Date: Friday, September 1, 2017

Issued Date: Friday, September 1, 2017