FMCSA-HOS-ELD-TECH-395-FAQ57(2022-03-10)

**Question:** Is the display required to be handed to the inspector outside of the vehicle?

**Guidance:** Under section 4.8.1.2 of [49 CFR part 395, subpart B, Appendix A](https://www.ecfr.gov/current/title-49/subtitle-B/chapter-III/subchapter-B/part-395#Appendix-A-to-Subpart-B-of-Part-395), if an electronic logging device (ELD) cannot produce a printout for use at roadside inspection, the display must be designed so that it can be reasonably viewed from outside the commercial motor vehicle (CMV). That may require the device to be untethered from its mount or connected in a manner that would allow it to be passed outside of the vehicle for a reasonable distance.

**Contact Info:** FMCSA ELD Information, 1-800-832-5660 or [ELD@dot.gov](mailto:ELD@dot.gov).

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

*Note: This guidance document does not have the force and effect of law and is not meant to bind the public in any way.  It is intended only to provide information and clarity regarding existing requirements under the law or agency policies.*

**Regulatory Topic: ELD Guidance**

Effective Date: Thursday, March 10, 2022

Issued Date: Thursday, March 10, 2022