FMCSA-HOS-ELD-TECH-395-FAQ65(2017-09-01)-CORR1

**Question:** What information should be displayed on the header for co-driver operations?

**Guidance:** The header should contain the information of the current co-driver. If there is no active co-driver at the time of inspection, then this field should be left blank. If a co-driver has been active during the record retention selection, the co-driver will be listed in the user list of the data transfer file. For the back-up print or display, providers may list the co-driver active for that day in the daily header.

**Contact Info:** FMCSA ELD Information, 1-800-832-5660 or [ELD@dot.gov](mailto:ELD@dot.gov).

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

*Note: This guidance document does not have the force and effect of law and is not meant to bind the public in any way. It is intended only to provide information and clarity regarding existing requirements under the law or agency policies.*

**Regulatory Topic: ELD Guidance**

Effective Date: Friday, September 1, 2017

Issued Date: Friday, September 1, 2017