FMCSA-HOS-ELD-TECH-395-FAQ70(2017-09-01)-CORR1

**Question:** As specified in section 4.8.2.1.1 of 49 CFR part 395, subpart B, Appendix A, the electronic logging device (ELD) output file must have one line for co-driver information and one line for commercial motor vehicle (CMV) information. How can the ELD account for multiple co-drivers and/or multiple CMVs?

**Guidance:** For files generated during roadside safety inspections, the active co-driver and CMV, must be reflected. For motor carrier data transfer (for compliance investigations), the ELD output file header should reflect the co-driver and CMV in use at the end of the requested time period.

In either case, the file must contain all administrative users, co-drivers, and CMVs referenced during the requested time period.

**Contact Info:** FMCSA ELD Information, 1-800-832-5660 or [ELD@dot.gov](mailto:ELD@dot.gov).

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

*Note: This guidance document does not have the force and effect of law and is not meant to bind the public in any way. It is intended only to provide information and clarity regarding existing requirements under the law or agency policies.*

**Regulatory Topic: ELD Guidance**

Effective Date: Friday, September 1, 2017

Issued Date: Friday, September 1, 2017