FMCSA-HOS-ELD-TECH-395-FAQ76(2017-09-01)-CORR1

**Question:** Regarding section 4.8.2.1.9 of 49 CFR part 395, subpart B, Appendix A, which power up and shut down events should be included?

**Guidance:** All power up and shut down events for all commercial motor vehicles (CMVs) used by the driver within the time period that is being requested should be included, including those events that belong to another driver (e.g., if the driver was not using that CMV on that day).

**Contact Info:** FMCSA ELD Information, 1-800-832-5660 or ELD@dot.gov.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

*Note: This guidance document does not have the force and effect of law and is not meant to bind the public in any way. It is intended only to provide information and clarity regarding existing requirements under the law or agency policies.*

**Regulatory Topic: ELD Guidance**

Effective Date: Friday, September 1, 2017

Issued Date: Friday, September 1, 2017