Top Cargo Tank Facility Violations

**Top Cargo Tank Facility Violations - 2017**

|  |  |  |
| --- | --- | --- |
|  | | |
| **PART NO** | **SECTION** | **DESCRIPTION** |
| 172 | 704(d) | Failing To Keep Training Records For 90 Days After Termination. |
| 172 | 704(c)(2) | Failing To Retrain Hazmat Employees Every Three Years. |
| 180 | 407(h) | Failing To Perform Leakage Test As Prescribed. |
| 180 | 407(d) | Failing To Perform An External Visual Inspection As Prescribed. |
| 172 | 704(a) | Failing To Train HM Employees As Required. |
| 172 | 704(a)(2) | Failing To Train HM Employee In Function Specific Training. |
| 180 | 409 | Failing to meet the Minimum Qualifications for Inspectors and Testers. |
| 107 | 503(a) | Failing To Include All Required Info In Registration Statement. |
| 107 | 504(d)(1) | Failing To Notify Within 30 Days Of Changes To Reg. Information. |
| 180 | 407(d)(7) | Failing To Record Required Info For External Visual Exam. |
| 107 | 502(b) | Manufacturing/Assembling/Etc. A Spec Tank Without Registering. |
| 171 | 2(g) | Cargo Tank Does Not Comply With HM Regulations. |
| 172 | 704(a)1 | Failing To Train HM Employee On General Awareness And Familiarization. |
| 172 | 704(a)4 | Failing To Provide Security Awareness Training. |
| 177 | 800(c) | Carrier Failed To Provide General Awareness/Familiarization Training |
| 180 | 407(g)(7) | Failing To Record Results Of Pressure Test. |
| 107 | 504(c) | Failing To Renew Registration When Required. |
| 107 | 504(e) | Failing To Maintain Current Copy Of Registration Information. |
| 180 | 407(i) | Failing To Perform A Thickness Test As Prescribed. |
| 180 | 407(e)(4) | Failing To Record Required Info On Internal Visual Inspection. |

**Top Cargo Tank Facility Violations - 2016**

|  |  |  |  |
| --- | --- | --- | --- |
| **PART NO** | **SECTION** | **DESCRIPTION** | |
| 180 | 417(b) | | Failing To Include All Required Information On Test/Inspection Report. |
| 180 | 407(g) | | Failing To Perform A Pressure Retest As Prescribed. |
| 172 | 704(c)(2) | | Failing To Retrain Hazmat Employees Every Three Years. |
| 172 | 704(d) | | Training requirements - Failing to keep training records for 90 days after termination. |
| 180 | 409 | | Failing To Meet The Minimum Qualifications For Inspectors Of Cargo Tanks. |
| 107 | 504(d)(1) | | Failing To Notify Within 30 Days Of Changes To Reg. Information. |
| 172 | 704(a)(2) | | Failing To Train HM Employee In Function Specific Training. |
| 180 | 407(d) | | Requirements for test and inspection of specification cargo tanks - Failing to perform an external visual inspection as prescribed |
| 107 | 504(e) | | Failing To Maintain Current Copy Of Registration Info. |
| 172 | 704(a) | | Training requirements - Failing To Train HM Employees As Required. |
| 107 | 503(a) | | Failing To Provide Security Awareness Training. |
| 171 | 2(g) | | Cargo tank does not comply with HM Regulations. |
| 180 | 407(h) | | Requirements for test and inspection of specification cargo tanks - Failing to perform leakage test as prescribed |
| 107 | 502(b) | | General registration requirements - Manufacturing/assembling/etc. spec tank without registering. |
| 180 | 407 (e) | | Failing To Perform Internal Visual Inspection |
| 180 | 407(h)(5) | | Failing To Record Results Of Leakage Test |
| 178 | 345(3)(f)(3) | | Except as prescribed in paragraphs (f)(1) and (f)(2) of this section, the welding of any appurtenance to the cargo tank wall must be made by attachment of a mounting pad. |
| 180 | 407(g)(7) | | Requirements for test and inspection of specification cargo tanks - Failing to record results of pressure test |
| 180 | 413(a) | | Any repair, modification, stretching, rebarrelling, or mounting of a cargo tank must be performed in conformance with the requirements of this section. |
| 180 | 415 | | Failing To Mark Test Date On Cargo Tank |

**Top Cargo Tank Facility Violations - 2015**

|  |  |  |
| --- | --- | --- |
| **PART NO** | **SECTION** | **DESCRIPTION** |
| 180 | 417(b) | Failing To Include All Required Information On Test/Inspection Report. |
| 172 | 704(d) | Failing To Keep Training Records For 90 Days After Termination. |
| 180 | 407(g) | Failing To Perform A Pressure Retest As Prescribed. |
| 172 | 704(c)(2) | Failing To Retrain Hazmat Employees Every Three Years. |
| 180 | 407(d) | Failing To Perform An External Visual Inspection As Prescribed. |
| 180 | 409 | Failing To Meet The Minimum Qualifications For Inspectors Of Cargo Tanks. |
| 172 | 704(a)(2) | Failing To Train HM Employee In Function Specific Training. |
| 180 | 407(h) | Failing To Perform Leakage Test As Prescribed. |
| 107 | 504(e) | Failing To Maintain Current Copy Of Registration Info. |
| 172 | 704(a) | Training requirements - Failing To Train HM Employees As Required. |
| 107 | 504(d)(1) | Failing To Notify Within 30 Days Of Changes To Reg. Information. |
| 180 | 407(a)(3) | Requirements for test and inspection of specification cargo tanks - Performing test/inspection w/o meeting minimum qualifications. |
| 107 | 502(b) | General registration requirements - Manufacturing/assembling/etc. spec tank without registering. |
| 107 | 503(a) | Failing To Provide Security Awareness Training. |
| 180 | 409 | Failing to meet the minimum qualifications for Inspectors of cargo tanks. |
| 180 | 409(a)(2) | Perform/Witness Inspect/Test On Cargo Tank W/O Training/Experience. |
| 180 | 415 | Failing To Mark Test Date On Cargo Tank. |
| 107 | 503(a) | Each registration statement must be in English and contain the required information - Failing to include all required info in registration statement. |
| 171 | 2(g) | Cargo tank does not comply with HM Regulations. |
| 180 | 407(i) | Requirements for test and inspection of specification cargo tanks - Failing to perform a thickness test as prescribed. |

**Top Cargo Tank Facility Violations - 2014**

|  |  |  |
| --- | --- | --- |
| **PART NO** | **SECTION** | **DESCRIPTION** |
| 180 | 417(b) | Failing To Include All Required Information On Test/Inspection Report |
| 180 | 407(g) | Failing To Perform A Pressure Retest As Prescribed |
| 172 | 704(c)(2) | Failing To Retrain Hazmat Employees Every Three Years |
| 172 | 704(d) | Failing To Keep Training Records For 90 Days After Termination |
| 172 | 704(a)(2) | Failing To Train Hazmat Employee In Function Specific Training |
| 180 | 407(d) | Failing To Perform An External Visual Inspection As Prescribed |
| 107 | 504(d)(1) | Failing To Notify Within 30 Days Of Changes To Reg. Info |
| 172 | 704(a) | Failing To Train HM Employees As Required |
| 172 | 704(c) | Failing To Train HM Employees As Required Initial And Recurrent Training |
| 180 | 3(a) | Representing As A Specification Package |
| 172 | 802(b) | Failing To Revise And Update Security Plan |
| 180 | 415 | Failing To Mark Test Date On Cargo Tank |
| 107 | 503(a) | Failing To Include All Required Info In Registration Statement |
| 173 | 315(m)(2)(vi) | Failing to Properly Mark A Nurse Tank In Accordance With §180.415(b) |
| 180 | 407(e) | Failing To Perform Internal Visual Inspection |
| 171 | 2(e) | Failing To Perform A Function Covered By An Exemption |
| 180 | 407(h) | Failing To Perform Leakage Test As Prescribed |
| 180 | 407(g)(3) | Failing To Perform Wet Fluor. Mag. Part. Test On Mc330/331 |
| 180 | 416(d) | Failing to conduct and record monthly inspections and tests |
| 180 | 407(a)(3) | Performing Test/Inspection W/O Meeting Min. Qualifications |

**Top Cargo Tank Facility Violations - 2013**

|  |  |  |
| --- | --- | --- |
|  | | |
| **PART NO** | **SECTION** | **DESCRIPTION** |
| 180 | 417(b) | Failing To Include All Required Information On Test/Inspection Report |
| 172 | 704(d) | Failing To Keep Training Records For 90 Days After Termination |
| 180 | 407(g) | Failing To Perform A Pressure Retest As Prescribed |
| 180 | 407(d) | Failing To Perform An External Visual Inspection As Prescribed |
| 172 | 704(a) | Training requirements - Failing To Train HM Employees As Required |
| 172 | 704(c)(2) | Failing To Retrain Hazmat Employees Every Three Years |
| 180 | 407(h) | Failing To Perform Leakage Test As Prescribed |
| 107 | 502(b) | Manufacturing/Assembling/Etc. A Spec Tank Without Registering |
| 107 | 503(a) | Failing To Include All Required Information In Registration Statement |
| 107 | 504(d)(1) | Failing To Notify Within 30 Days Of Changes To Reg. Information |
| 172 | 704(a)(1) | Failing To Train HM Employee On General Awareness And Familiarization |
| 172 | 704(a)(2) | Failing To Train HM Employee In Function Specific Training |
| 180 | 407(g)(1)(iv) | Failing To Perform Hydrostatic Test At Required Pressure |
| 180 | 407(g)(3) | Failing To Perform Wet Fluorescent Magnetic Particle Testing On MC 330/331 Cargo Tanks |
| 180 | 409 | Failing to meet the minimum qualifications for Inspectors of cargo tanks |
| 107 | 504(a) | Failing To Renew Registration Every 6 Years |
| 172 | 704(a)(4) | Failing To Provide Security Awareness Training |
| 180 | 407(d)(7) | Failing To Record Required Information For External Visual Exam |
| 180 | 407(h)(5) | Failing To Record Results Of Leakage Test |
| 107 | 504(e) | Failing To Maintain Current Copy Of Registration Information |

**Top Cargo Tank Facility Violations - 2012**

|  |  |  |
| --- | --- | --- |
|  | | |
| **PART NO** | **SECTION** | **DESCRIPTION** |
| 180 | 417(b) | Failing to include all required information on test/inspection report |
| 172 | 704(c)2 | Failing To Retrain Hazmat Employees Every Three Years |
| 172 | 704(d) | Failing To Keep Training Records For 90 Days After Termination |
| 172 | 704(a) | Failing To Train HM Employees As Required |
| 180 | 407(g) | Failing To Perform A Pressure Retest As Prescribed |
| 172 | 704(a)(2) | Failing To Train HM Employee In Function Specific Training |
| 107 | 504(d)(1) | Failing To Notify Within 30 Days Of Changes To Reg. Information |
| 171 | 2(g) | Cargo tank does not comply with HM Regulations |
| 107 | 502(b) | Manufacturing/Assembling/Etc. A Spec Tank Without Registering |
| 180 | 407(d) | Failing To Perform An External Visual Inspection As Prescribed |
| 180 | 407(h) | Failing To Perform Leakage Test As Prescribed |
| 107 | 504(e) | Failing To Maintain Current Copy Of Registration Info |
| 172 | 704(a)(1) | Failing To Train HM Employee On General Awareness And Familiarization |
| 172 | 704(a)(4) | Failing To Provide Security Awareness Training |
| 180 | 409 | Failing to meet the minimum qualifications for Inspectors of cargo tanks |
| 180 | 409(a)(2) | Perform/Witness Inspect/Test On Cargo Tank W/O Training/Experience |
| 180 | 415 | Failing To Mark Test Date On Cargo Tank |
| 107 | 503(a) | Failing To Include All Required Info In Registration Statement |
| 107 | 504(a) | Failing To Renew Registration Every 6 Years |
| 107 | 608(a) | Failing To Register With Department |

**Top Cargo Tank Facility Violations - 2011**

|  |  |  |
| --- | --- | --- |
|  | | |
| **PART NO** | **SECTION** | **DESCRIPTION** |
| 180 | 417(b) | Failing to include all required information on test/inspection report |
| 180 | 407(d) | Failing to perform an external visual inspection as prescribed |
| 180 | 407(g) | Failing To Perform A Pressure Retest As Prescribed |
| 107 | 503(a) | Failing To Include All Required Info In Registration Statement |
| 180 | 407(h) | Failing To Perform Leakage Test As Prescribed |
| 107 | 504(c) | Failing To Renew Registration When Required |
| 107 | 504 (d)(1) | Failing To Notify Within 30 Days Of Changes To Reg. Info |
| 107 | 504 (e) | Failing To Maintain Current Copy Of Registration Info |
| 171 | 2(g) | Cargo tank does not comply with HM Regulations |
| 180 | 407 (g)(1)(iv) | Failing To Perform Hydrostatic Test At Required Pressure |
| 180 | 409(a)(2) | Perform/Witness Inspect/Test On Cargo Tank W/O Training/Experience |
| 107 | 502(b) | Manufacturing/Assembling/Etc. A Spec Tank Without Registering |
| 107 | 504(a) | Failing To Renew Registration Every 6 Years |
| 180 | 407 (e) | Failing To Perform Internal Visual Inspection |
| 180 | 409 | Failing to meet the minimum qualifications for Inspectors of cargo tanks |
| 180 | 409d3 | Doing Pressure Retest, Not Keeping Copy Of Tester Qualification |
| 180 | 413 (a)(1) | Failing to perform repair to DOT spec cargo tank in accordance w/ NBIC in effect |
| 180 | 413 (a)(1)(i) | Performing repair - non-ASME cargo tank w/o "R" or "U" stamp |
| 107 | 504(d)(2) | Failing To Notify Within 30 Days Of Replacing Person |
| 107 | 608(a) | Failing To Register With Department |

**Top Cargo Tank Facility Violations - 2010**

|  |  |  |
| --- | --- | --- |
|  | | |
| **PART NO** | **SECTION** | **DESCRIPTION** |
| 180 | 417(b) | Reporting and record retention requirements - Failing to include all required information on test/inspection report |
| 180 | 407(g) | Requirements for test and inspection of specification cargo tanks - Failing to perform a pressure retest as prescribed |
| 172 | 704(d) | Training requirements - Failing to keep training records for 90 days after termination |
| 172 | 704(a) | Training requirements - Failing to train HM employees as required |
| 172 | 704(c)(2) | Training requirements - Failing to retrain Hazmat employees every three years |
| 172 | 704(a)(2) | Training requirements - Failing to train HM employee in function specific training |
| 107 | 504(e) | Period of registration, updates, and record retention - Failing to maintain current copy of registration information |
| 180 | 409 | Minimum qualifications for inspectors and testers - Failing to employ inspectors and testers with the minimum qualifications |
| 107 | 504(d)(1) | Period of registration, updates, and record retention - Failing to notify within 30 days of changes to reg. information |
| 180 | 407(a)(3) | Performing test and/or inspection without meeting minimum qualifications |
| 180 | 407(d) | Requirements for test and inspection of specification cargo tanks - Failing to perform an external visual inspection as prescribed |
| 180 | 407(h) | Requirements for test and inspection of specification cargo tanks - Failing to perform leakage test as prescribed |
| 107 | 503(a) | Each registration statement must be in English and contain the required information - Failing to include all required info in registration statement |
| 107 | 502(b) | General registration requirements - Manufacturing/assembling/etc. a spec tank without registering |
| 107 | 504(a) | Period of registration, updates, and record retention - Failing to renew registration every 6 years |
| 107 | 502(d)(2) | Period of registration, updates, and record retention - failing to notify within 30 days of replacing person |
| 172 | 704(a)(1) | Training requirements - Failing to train hazmat employee on general awareness and familiarization |
| 180 | 407(h)(4) | Requirements for test and inspection of specification cargo tanks - Failing to inspect and record delivery hose/piping inspection |
| 107 | 504(c) | Period of registration, updates, and record retention - Failing to renew registration when required |
| 180 | 416(d)(5) | Discharge system inspection and maintenance program for cargo tanks transporting liquefied compressed gases - No complete record of monthly discharge system inspection and test |

**Top Cargo Tank Facility Violations - 2009**

|  |  |  |
| --- | --- | --- |
|  | | |
| **PART NO** | **SECTION** | **DESCRIPTION** |
| 180 | 417(b) | Reporting and record retention requirements - Failing to include all required information on test/inspection report |
| 172 | 704(d) | Training requirements - Failing to keep training records for 90 days after termination |
| 172 | 704(a) | Training requirements - Failing to train HM employees as required |
| 107 | 502(b) | General registration requirements - Manufacturing/assembling/etc. a spec tank without registering |
| 180 | 407(d) | Requirements for test and inspection of specification cargo tanks - Failing to perform an external visual inspection as prescribed |
| 107 | 504(e) | Period of registration, updates, and record retention - Failing to maintain current copy of registration information |
| 180 | 417(a)(1) | Reporting and record retention requirements -Vehicle certification - Failing to maintain copies of required certificate and papers owner |
| 107 | 503(a) | Each registration statement must be in English and contain the required information - Failing to include all required info in registration statement |
| 172 | 704(a)(2) | Training requirements - Failing to train HM employee in function specific training |
| 172 | 704(c)(2) | Training requirements - Failing to retrain Hazmat employees every three years |
| 396 | 17(a) | Periodic inspection - Using a CMV not periodically inspected |
| 180 | 407(g) | Requirements for test and inspection of specification cargo tanks - Failing to perform a pressure retest as prescribed |
| 172 | 802(a) | Components of a security plan - Security plan does not contain risk assessment |
| 172 | 704(a)(5) | Training requirements - Failing to provide in-depth security awareness training |
| 180 | 416(d)(5) | Discharge system inspection and maintenance program for cargo tanks transporting liquefied compressed gases - No complete recd. of monthly discharge system insp. & test |
| 177 | 840(l) | Class 2 (gases) materials - No written emergency discharge procedures - compressed gas |
| 180 | 407(h) | Requirements for test and inspection of specification cargo tanks - Failing to perform leakage test as prescribed |
| 180 | 409(d)(3) | Minimum qualifications for inspectors and testers - Doing pressure retest, not keeping copy of tester qualification |
| 107 | 504(d)(1) | Period of registration, updates, and record retention - Failing to notify within 30 days of changes to reg. information |
| 180 | 409 | Minimum qualifications for inspectors and testers - Failing to employ inspectors and testers with the minimum qualifications |

**Top Cargo Tank Facility Violations - 2008**

|  |  |  |
| --- | --- | --- |
|  | | |
| **PART NO** | **SECTION** | **DESCRIPTION** |
| 180 | 417(b) | Reporting and record retention requirements - Failing to include all required information on test/inspection report |
| 172 | 704(d) | Training requirements - Failing to keep training records for 90 days after termination |
| 172 | 704(a) | Training requirements - Failing to train HM employees as required |
| 180 | 407(g) | Requirements for test and inspection of specification cargo tanks - Failing to perform a pressure retest as prescribed |
| 180 | 407(d) | Requirements for test and inspection of specification cargo tanks - Failing to perform an external visual inspection as prescribed |
| 107 | 504(e) | Period of registration, updates, and record retention - Failing to maintain current copy of registration information |
| 180 | 407(h) | Requirements for test and inspection of specification cargo tanks - Failing to perform leakage test as prescribed |
| 107 | 503(a) | Each registration statement must be in English and contain the required information - Failing to include all required info in registration statement |
| 172 | 704(c)(2) | Training requirements - Failing to retrain Hazmat employees every three years |
| 107 | 504(c) | Period of registration, updates, and record retention - Failing to renew registration when required |
| 180 | 407(a)(3) | Requirements for test and inspection of specification cargo tanks - Performing test/inspection w/o meeting minimum qualifications |
| 180 | 407(c) | Requirements for test and inspection of specification cargo tanks - Failing to periodically test and inspect cargo tank |
| 107 | 504(d)(1) | Period of registration, updates, and record retention - Failing to notify within 30 days of changes to reg. information |
| 180 | 417(a)(1) | Reporting and record retention requirements -Vehicle certification - Failing to maintain copies of required certificate and papers owner |
| 180 | 407(i) | Requirements for test and inspection of specification cargo tanks - Failing to perform a thickness test as prescribed |
| 107 | 504(d)(2) | Period of registration, updates, and record retention - Failing to notify within 30 days of replacing person |
| 180 | 409 | Minimum qualifications for inspectors and testers - Failing to employ inspectors and testers with the minimum qualifications |
| 107 | 504(d)(4) | Period of registration, updates, and record retention - Failing to notify within 30 days of change in function |
| 180 | 407(g)(7) | Requirements for test and inspection of specification cargo tanks - Failing to record results of pressure test |
| 180 | 407(h)(4) | Requirements for test and inspection of specification cargo tanks - Failing to inspect and record delivery hose/piping inspection |